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	Description:

	Connector Lead for Lighting Circuits

	5 Core x 2.5mm²

	Low Fire Hazard (XLPE) Cable

	Cable Colour:
	Black



Please read instructions before commencing installation and retain for future reference.




Technical Specification: 
	Material:
	Connector:

	
	PA66 + 25% GF UL-94 V0 (S/N 704872-1)

	
	PA66 unfilled UL-94 V2 (S/N 1573372-1)

	Connector Dimensions:
	56mm (L) x ø 24mm (W)

	Cable Insulation:
	HFS-90-TP Sheath (BK)

	Cable Rating:
	450/750V to AS/NZS 5000.2

	Minimum Bending Radius:
	Fixed: 70mm

	
	During Installation: 110mm 

	Overall Cable Diameter:
	12.2mm

	Maximum Operating Temperature:
	90°C

	Enclosure Class:
	IP20

	Rated Current (A):
	16A

	Power Outputs:
	6 Pole (5 Wire)

	Rated Voltage (V):
	240V

	Frequency (Hz):
	50Hz

	Wire Size (mm²)
	2.5mm²

	Weight:
	272g (based on 1m)

	Wiring & Test Standard:
	AS/NZS 3000

	Connector Coupler Standard:
	AS/NZS 61535:2011
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